Spatial information about the 9 sites:
X_Lambert 93;Y_Lambert 93;altitude;land use
818574;6388501;298;fallow land in limestone
818887;6387840;265;little steep vineyard
818781;6387727;263;small oak wood with grassland
818905;6388519;282;small truffle oaks wood with grassland
818760;6387477;259;permanent pasture
818742;6388013;263;steep vineyard
822662;6397782;740;foothill pasture
822630;6397794;743;tophill pasture
822555;6397574;736;south faced pasture


The metadata are described at http://mistrals.sedoo.fr/?editDatsId=1350.


In "soil_moisture_network_metadata.xls" the following information are given :
-the real depths of the 5 sensors at each site
-the probe ID of each sensor
-the land use ID for each site

"soil_moisture_sensor_network.csv" is the time series of soil moisture for the five sensors at each site.
File Header Abbreviations:
* Theta: value of volumetric water content (% Volume)
* Date_Time: date format dd/mm/yyyy hh:mm
* Location: land use ID
* Depth_real: real depth of the sensor (in cm)
* Depth_class: class of depth of the sensor: 10 cm, 25 cm or 40 cm
* Land_Use: dominant land use
* Probe_id: identification number of the sensor


More information are available in the MSc Thesis Report of Magdalena Uber (2016).
